|  |  |  |
| --- | --- | --- |
| # | Question | Answer |
| 1 | Is there any study for borehole included drilling? | Yes, a geophysical survey has been done and the recommendation is to use combined drilling machine to drill the borehole. |
| 2 | What are the borehole casing diameters? | This is well defined in the drilling TOR attached with RFQ documents as below:  1. Using the recommendation of the geophysical survey report or otherwise instructed by GOAL field supervising engineer the contractor should drill to the recommended depth of 60-70 meter with a diameter of 10 ¾’’- 14’’  2. Installation of standard 8 5/8’’ diameter steel pipe ASTM or API or UPVC pipe not less than 10 bar per inch to the agreed Depth. Steel pipe of other brand should be coated with standard coat inside and outside the pipe |
| 3 | What is the type of Pipe? 12 meter or by Roll? | Both types are accepted |