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TOR Water Trucking Services to Transit, Port Sudan Country Office

[bookmark: _GoBack]Request for Quotation Form

World Vision Sudan (WVS)invites proposals to offer water trucking services to its facilities and drinking bottled Jars in Port Sudan.

NOTE: - 
1. Kindly indicate delivery lead times (MUST). 
2. Prices should be Inclusive of applicable government taxes. 
3. Only successful bidders will be contacted 
4. Our payment terms are 30 days of Credit. 
5. Quotation price should be in SDG or USD

A. PRELIMINARY REQUIREMENT 

To qualify for award of the Contract, bidders shall meet the following minimum qualifying criteria; 
Eligible bidders should attach valid documentation and be able to meet the following minimum requirements:- 
1. Must be a registered company (Attach Certificate of Incorporation) 
2. Indicate source of water in Port Sudan
3. Sudan Government relevant permits
4. Valid water quality analysis report for both physical, biological and chemical parameters (should be within Sudan drinking water standards), the test should be done every 3 months and the report to be shared with WVS timely. 
5. Please take note of the requirements below which form part of the instructions for this tender; 
· Water tankers should only get their water from approved sources preferably through a hydrant provided, controlled and designated as a source by the state water corporation 
· Water tankers should only get their water from sources where Water is treated at the source ensuring no physical, biological or chemical contamination in the water preferably from Hala (حلا) water treatment station 
· The abstraction methods chosen by water vendors should not lead to contamination of the water. Pumps and hosepipes used should be kept clean. 
· The tankers should have proper fitting covers which should always be kept closed. 
· Water tankers should be thoroughly cleaned, disinfected and inspected regularly. 
· Vendor must practice good personal hygiene so as not to contaminate water they are vending. 
· Personnel involved in handling the water should have a health clearance certificate from MoH 
· Please note that if awarded, the water tankers used to supply water must not be used for anything other than supply of water. Contravention of this requirement will lead to immediate cancelation of the order and possible legal action. 
· Old and rusted tankers should not be used to supply water to World Vision 
6. Please take note of the requirements below for bottled jars of drinking water 
· The supplier warrants those water jar supplied under this agreement is packed properly.
· All goods shall be delivered to World Vision Sudan in their original manufacturers packaging     
· WV Sudan shall have reasonable time during delivery to conduct physical verification
REQUIREMENT
	
	Description
	Sites
	Unit

	Quantity
	Unit Price
	Total Amount

	1
	Supply of Water 30,000 Litre capacity Water Tanker. May refill on a Weekly basis

	Transit area 
	Trip
	1
	
	

	2
	Bottled Drinking Water –18 Litre Jar
300 - 350 Jars / Month
	Transit area
	Jar
	1
	
	




7. Duration of the Assignment:
The entire assignment will run for 12 Months from date of signing of the contract.
7-Reporting and Supervision:
The Contractor will work under the direct supervision of and report to Administration Unit. 
All deliverables must be submitted to Administration Office for review and formal approval.
8-Payment Schedule:
Payments will be made in 30 days credit period after invoice submission based on deliverables
100% upon successful completion of tangible deliveries and submission of the Tracking Report.
9. Contact Information:
For inquiries and bid submission, please contact:
	S/NO
	Position
	Email

	1
	Secretariat, Procurement Committee, World Vision Sudan
	scm_sudan@wvi.org
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