
	Name of Tender:
Rehabilitation of Sheria, Bahar Alarab and Abojabra SCs in ED.
1. Repair Abu Jabra SC the existing room, construct a kitchen by local materials and to use room for nutrition assistants to provide table for milk preparation supported by kitchen set , extension of ward , connect to a water supply as per BoQ.

2. Repair Bahar Alarab SC rooms, repair the existing latrine, repair the medical waste incinerator, connect to a water supply build a kitchen with local material, Zink, Rehabilitation of west management per BoQ.


3. Repair Sheria SC rooms, connect to a water supply, construct a kitchen with local materials , repair the existing latrine, install a solar power system. Rehabilitation of west management as per BoQ.
4. Provide and installing of solar system I (Abu jabra, Bahar Alarab and Sheria SCs) includs Battary 5k, solar panel 550W, 8 pannels, Inverter 5k , all accessories per BoQ.
   Tender Number 
SD-CRS-538604-CW-RFQ
 Publish date 19th of October 2026  
Deadline Submission date:
 2nd November 2026 – 04 :00 PM
Please submit your bid to CRS El Daein or through E/mail 
tenders.sudan@crs.org  

  









	اسم العطاء:
تنفيذ أعمال إعادة تأهيل وتحسين البنية التحتية لمراكز الاستقرار في  شعيرية, بحر العرب, و ابوجابرة   ولاية شرق دارفور بما في ذلك إدارة النفايات. 
1. صيانة غرف مركز الاستقرار ابوجابرةو بناء مطبخ من المواد المحلية و الزنك و توفير تربيزة لتجهيز اللبن للاطفال مع توفير اطقم اواني و توصيل المياه
2. صيانة غرف مركز الاستقرار بحر العرب و صيانة المرحاض و محرقة النفايات وبناء مطبخ من المواد المحلية و الزنك و توصيل المياه
3. صيانة غرف مركز الاستقرار شعيرية و صيانة المرحاض و محرقة النفايات وبناء مطبخ من المواد المحلية و الزنك و توصيل المياه
4. توريد مواد و تركيب نظام طاقة شمسية في الثلاثة مراكز حسب جدول التقديرات المرفق

رقم العطاء
  SD-CRS-538604-CW-RFQ
تاريخ فتح التقديم:  19 اكتوبر 2026 
 
تاريخ انتهاء التقديم 

2 نوفمبر 2026 04:00   العصر 
 
 
 الرجاء ارسال عرضكم الي مكتب الاغاثة الكاثلوكية فى الضعين, زالنجي, او من خلال البريد الالكتروني 
tenders.sudan@crs.org 














 
 
	Dear Sir / Madam, 
CRS Sudan is looking for companies for Rehabilitation of Sheria, Bahar Alarab and Abojabra SCs in East Darfur.
 
General Requirements 
1.  Must Be Registered to conduct the business and in compliance with federal governments tax regulations in Sudan.
2.     Past Eexperience with International Organizations, Non-Governmental Organizations, or large private companies will be an added advantage.  
4.   CRS retains the right to reject, cancel, negotiate, amend, split and accept any offer, without consideration of the lowest offer. 
5.     This is an invitation to vendors, and it is not a promise or obligation that CRS will contract with suppliers through the submitted offers.
6.   Relevant bid committee may request for physical samples of some items during evaluation process of bids. 
7. The work plan must be provided by the contractor with the tender package.
9.The banking information should be specific and clear.


	 سيدي / سيدتي العزيز(ة)
هيئة الإغاثة الكاثوليكية  برامج السودان تبحث عن شركات من المهتمين تنفيذ أعمال إعادة تأهيل وتحسين البنية التحتية لوحدة شعيرية, بحر العرب, و ابوجابرة  بما في ذلك إدارة النفايات. في ولاية شرق دارفور
متطلبات عامة:
1 . يجب أن يكون مسجلا لإجراء الأعمال التجارية مع ما يتوافق  ولوائح الضرائب الحكومية في السودان .
3 . الخبرة في تزويد المنظمات الدولية، المنظمات الغير حكومية، أو  الشركات الكبيرة الخاصة ستكون ميزة.
4 . تحتفظ هيئة الاغاثة الكاثوليكية بالحق في رفض، إلغاء، التفاوض، تعديل، تجزئة وقبول أي عرض، دون النظر الى أدنى عرض. .
5. هذه دعوة للموردين وليس وعد أو التزام من هيئة الإغاثة الكاثوليكية للتعاقد مع الموردين من خلال العروض المقدمة
6. قد تقوم لجنة الإحالة المعنية بطلب نماذج عينية لبعض المواد اثناء عملية تقييم العروض.
7.  يجب على المقاول تحضير الجدول الزمني لتنفيذ الاعمال على ان يتم تسليم المستند مع اوراق العطاء
9. يجب ان تكون معلومات وتفاصيل رقم الحساب واضحة.



 
	Payment Terms
1. Quotation should remain valid for a period of at least sixty (60) days from the submission closing date. 
2. Payment shall be made in SDG via bank cheque or wire transfer within 15 working days from the date of receiving the correct invoice.
3. Payment shall be made upon verification and acceptance of services/goods according to contract    Purchase order. 

	     شروط الدفع :- 
يجب أن تظل العرض ساريًا لمدة تصل إلى ستين (60) يومًا من تاريخ إغلاق التقديم.1
2. يتم إجراء الدفع بالحنيه السوداني عبر شيك بنكي أو تحويل بنكي خلال خمسة عشر (15) يوم عمل من تاريخ استلام الفاتورة الصحيحة.
3. يتم إجراء الدفع بعد التحقق وقبول الخدمات وفقًا لشروط العقد أو أمر الشراء





	Acceptance of Payment Terms
Do you accept the above payment terms?
· Yes
· No
 
	الموافقة على شروط الدفع:
هل توافق على شروط الدفع اعلاه:
· اوافق 
· لا اوافق 

	Requested Information
The submission must include:
· Full legal address and contact details of the company.
· Name of company’s official owner and copy of his/her ID & passport (if available)
· Copy of company registration certificate 
· Copy of Tax Registration Certificate.
· Reference from previous similar business experience with reference contact information. 
· Bank account information if available.
· The vendor must read, sign & stamp the Attachment (2) related to CRS SUPPLIER CODE OF CONDUCT
	يجب تقديم ما يلي:    
 يجب ان يتضمن التقديم ما يلي :                  
· العنوان الكامل الصحيح وعنوان الاتصال للشركة
· اسم صاحب الشركة الرسمي مع  نسخة من البطاقة القومية او جواز السفر.
· صورة عن شهادة تسجيل الشركة
· صورة عن شهادة التسجيل الضريبي 
· المرجع من الخبرة في الاعمال السابقة المماثلة و معلومات الاتصال للمرجع
· تفاصيل معلومات الحساب المصرفي اذا امكن.
· يجب على المقاول قراءة و توقيع و ختم الملحق(2) و الخاص بالقواعد السلوكية التي تنتهجها هيئة الإغاثة الكاثوليكية.


 
 
	Bid Requirements: - 
Offers that do not meet the following will be automatically rejected regardless of price:
1. Offers must be received before the stated deadline. 
2. Offers must include all the information requested above. 
3.  Unit prices must be provided for all line items. Offers that only include totals will be rejected.
4. Bids that include mistakes in calculations within the Bill of Quantities will be excluded from competition. 
5. Bids must be submitted through CRS Offices El Daein, Zalingei or EL Geneina office to receive bids. 
6. Offers must be clean & clear. The vendor should sign and stamp against any handwritten corrections/amendment to the bid. 
7. Offers must be, signed, dated, and stamped on all pages. 
8. The technical adviser of CRS will carry out quality control of the items and reserve the right to reject items that do not match the above-mentioned specification.
9. The duration of delivery for all requested items must be clearly specified 
	     
      معلومات ملء العطاء :- 
      سوف يتم رفض أي عطاء لا يلتزم بالشروط أدناه بغض النظر عن السعر:
1. سيتم رفض أي طلب يقدم بعد التاريخ والوقت المحدد لقبول العطاءات.
2. يجب أن تتضمن العروض جميع المعلومات المطلوبة أعلاه.
3. جميع الاسعار يجب ان تكتب لكل بند أو فقرة على حدة، ويتم رفض العطاءات التي تحتوي على الإجمالي فقط. 
4. سيتم استبعاد العطاء الذي يتضمن خطأ في حسابات جداول الكميات
5.  يجب تقديم العروض في مكتب المنظمة زالنجي  او الجنينة
6. العروض يجب أن تكون نظيفة وواضحة، يجب التوقيع والختم ان وجد في مكان أي تصحيح يدوي أو باستخدام قلم التصحيح الابيض.
7. يجب أن تكون العروض كاملة من جميع الجوانب، موقعة بتاريخ واضح ومختومة على جميع الصفحات.
8. سيقوم الجهة الفنية من قبل المنظمة لمطابقة المواصفات ويتم رفض أي دواء غير متطابق للمواصفات أعلاه.
9. يجب تحديد بشكل واضح  فترة تسليم كل الكميات المطلوبة 



 
	Delivery Instructions: 
1. The company biography should not exceed 10 pages.
  
Complete and stamped and signed offer must be delivered in sealed envelope with tender number on it 
SD-CRS-538604-CW-RFQ
Delivery to CRS El Daein or through E/mail 
tenders.sudan@crs.org 









	تعليمات التسليم: 
يجب ان لا تتجاوز السيرة الذاتية للشركة اكثر من 10 صفحات.
 
يجب تقديم العطاء الكامل والمختوم و الموقع  مع كافة الوثائق المطلوبة في  ظرف مغلق يكتب عليه رقم العطا 
  SD-CRS-538604-CW-RFQ
ويسلم الى مقر مكتب الاغاثة الكاثلوكية الضعين او من خلال البريد الالكتروني 
tenders.sudan@crs.org 
 











Experience Reference List
قائمة مراجع الاعمال السابقة
	  
	Name of Organization
أسم
المنظمة
	Name of Person
أسم الشخص
	Name of Project أسم المشروع
	Project Start Date تاريخ المباشرة بالمشروع
	Project duration مدة تنفيذ المشروع
	Phone Number رقم الموبايل
	Email Address البريد الالكتروني

	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 

	
	
	
	
	
	
	
	

	Company name:
أسم الشركة :
	  

	Legal address:
العنوان الثابت:
	  

	Telephone Number:
رقم الهاتف:
	  

	Email:
عنوان البريد الإلكتروني:
	 
 

	Representative Name
اسم الممثل:
	 
 

	Business Certificate Registration Number:
رقم تسجيل شهادة العمل:
	 

	Tax registration Number:
رقم التسجيل الضريبي:
	 

	Contract duration:
مدة العقد :
	 

	   Bank details: -

· Bank Name: ……………………………………
· Bank account name: …………………………
· Bank number ………………………………
· Branch: ………………………………………



  
	تفاصيل الحساب:- 

   إسم الينك : ----------------------------------------
 اسم الحساب :----------------------------------------
رقم الحساب :  --------------------------------------  
الفرع -----------------------------------------------


	Do you have partnerships with any other companies (such as shared management / staff / office / bank account)?  Do you cooperate with any other companies in preparing offers or providing goods or services?
هل لديك شراكات مع أي من الشركات الأخرى ( مثل إدارة / الموظفين / المكتب حساب مشترك / البنك) ؟ هل تتعاون مع أي من الشركات الأخرى في إعداد العروض أو توفير السلع أو الخدمات؟
	 

	If the answer to the above question is yes, please provide details here including the names of partner companies.
إذا كان الجواب عن السؤال السابق نعم ، يرجى تقديم التفاصيل هنا بما في ذلك أسماء الشركات الشريكة 
	 

	Other comments:
ملاحظات اخرى: 
	 

	Experience / references for the related work of experience (Please attached any related contract, purchase order, certificate, etc.) that does not exceed 10 pages. References MUST include contact information.  
يجب ان يحتوي على عناوين الاتصال من مراجع الخبرة 
المرجع من الخبرة ( الرجاء ارفاق دليل من الاعمال السابقة ذات الصلة من عقود , اوراق شراء , ورقة اتمام عمل , اخرى )  لا تتجاوز عشرة اوراق.
	 
 
 
 
 



	Signature
التوقيع
	 

	Date
التاريخ
	 











ATTACHED (1)
Lot#1 Abojabra SC
Bill Of Quantities for Repair Abu Jabra SC the existing room, construct a kitchen by local materials and to use room for nutrition assistants to provide table for milk preparation supported by kitchen set , extension of ward , connect to a water supply

	Construction room Abojabra:

	No
	Description
	Unit
	Qty
	U. Price USD
	Total USD

	1
	Site cleaning,
	L.S
	1
	
	

	2
	Provide and construct the Project sign-board ,fabricated from 4" circular steel pipe as stands height 1.5, casted by concrete with required depth (50cm) , well welded with heavy sheets 1mm thickness, 150cm*100cm for width and height respectively. All the components should be painted (one face anti-rust paint + two faces steel paints). All the Project information should be written on the sign-board based on the supervisor's instructions.
	L.S
	1
	
	

	3
	Excavate 60cm width 6cm deep strip foundation trench 
	ML
	28
	 
	 

	4
	Provide and build 60 cm depth of 2.5 brick strip foundation of first class ordinary burnt red clay brick  c/s mortar 1:6 with proper curing for three days.
	ML
	28
	
	

	5
	Provide and build 50 cm hight of 2brick (Gassa) of first class ordinary burnt red clay brick  c/s mortar 1:6 with proper curing for three days.
	ML
	28
	
	

	6
	Back filling for ground floor with selected material  fine sand (safaya sand) approved by the supervisor, filling material shall be clean and in layers not exceeding 200 mm watered and will compacted. as per the specification 
	M³
	24
	
	

	7
	Provide and build 1 (one) brick wall for the long spans of the two room total height 1.2m, of first class ordinary burnt red clay brick in c/s ,polyester work every 2 meters, mortar 1:6 with proper curing for three days.
	M²
	10
	
	

	8
	Provide and build 1.5  brick wall for the short spans of the shelter  to reach a Clean elevation of 4m inclouding the Barabate ,with  tie the new wall to the existing wall of the fance by interlocking the bricks courses with the existing wall   .Should use first class ordinary burnt red clay brick in c/s , polyester work every 3 meters , mortar 1:6 with proper curing for three days.
	M²
	48
	
	

	9
	Provide and construct heavy steel pipe 4*8cm of 1mm thickness, as columns(1.5m c/c) ,and roof rafters (1.5m c/c) with trusses, including all the necessary welding work as per the job specification and the required paints (one face anti-rust paints + two faces oily paints), the foundation of the steel pipes should be casted by concrete with required depth (50cm) and the cleared height should be 3.5 m(the higher side elevation 4m) from the NGL (Gassa).
	ML
	96
	
	

	10
	Provide and construct heavy steel pipes 3*6cm of 1mm thickness for roof and bracing  (Miraya), including all the necessary welding work as per the job specification and the required paints (one face anti-rust paints + two faces oily paints), the spacing should be 0.9m.
	ML
	104
	
	

	11
	Provide and fix metallic corrugated sheet 0.35mm for the roof with an adequate slope as per the drawings and specifications, as well as the remained wall  (Miraya) using the necessary and required stainless steel bolts with all it's accessories .
	M²
	52
	
	

	12
	 provide and install Heat  insulater for zinc roof sheets according  to the  Satisfaction  of the engineer
	M²
	48
	
	

	13
	Provide and install  doors 120*2.2m manufactured of Heavy 3*6 cm  pipes and heavy metallic sheet 0.8 mm  including all necessary welding work  and it's accessories (handle,lock,fiberglass,...) as well as  the required paints (one face anti-rust paint + two faces oily paints),as per the detailes and drawings .
	pcs
	1
	
	

	14
	Provide and install  windows 90*120cm , manufactured of Heavy 3*6 cm  pipes and heavy metallic sheet 0.8 mm including all necessary welding work and it's accessories (handle,lock,fiberglass,...) as well as  the required paints (one face anti-rust paints + two faces oily paints)
	pcs
	7
	
	

	15
	Provide and cast plain concrete 8 cm for the rooms well-leveled and well-watered 1:3:6 mix.
	M²
	48
	
	

	16
	provide and construct brick masonary staps at room enterance including all the finishing according to the engineer instructions 
	job
	1
	
	

	17
	provide material and install taile (ceramic size 40*40)inclouding the ( wazer 10 thichness)
	M²
	48
	
	

	18
	Provide 20mm sand cement mortar1:6 for external and internal plastering of the walls.
	M²
	126
	
	

	19
	 Cover  the internal areas from elevation 2.3m to the top of shelter[miraya] for both long spans , by heavy American zinc including all the necessary items and work[connections,steel nails] to be fixed properly
	M²
	37
	
	

	20
	Internal and external finishing painting  for the walls (three faces use pomaatic))with CRS Logo based on the supervisor's instructions.
	M²
	142
	
	

	21
	construction of local kitchen ( karank)  with dimention (  4*6*3m wide ,lenght,hight) using local materials wooden poles(sha,ab) , bamboo stick (cane) , grass mats (Sharghani) , bamboo sheet (haseer ) and all necessary local materials for complete construction including fabrication and installation of one door made from local materials ( bamboo).roof covering with heavy plastic sheet  to prevent rainwater penetration , complete with all labor ,tools transportation , fixing and every thing required for afully completed kitchen according  to the  Satisfaction  of the engineer .
	Job
	1
	
	

	Latrine & Incinerator Abojabra:

	22
	Excavate latrine hole dimensions (3*2.5*3m) length, width and depth and remove the soil away from the site.
	M³
	22.5
	
	

	23
	provide materials& labor cost & casting fabricate plain concrete at the bottom of the hole with dimension 3*2.5*.1m [length, width and thickness] using cement , sand,gravel with ratio  1:3:6 
	M²
	7.5
	
	

	24
	Provide materials & cast reinforcement concrete for G beam dimensions (.3*.3*11m) with reinforcement concrete ratio 1:2:4 by using 6 bars 12mm  and steel bars  6mm 15cm c/c .
	ML
	11
	
	

	25
	Provide materials and build supporting wall from red bricks  no 1 ,  1.5 brick thickness , by using cement nortar 1:6  and with internal  plasetring by using cement mortar 1:6 and grey painting (rifcot).
	M²
	36
	
	

	26
	Provide materials and cast reinforcement concrete for ring beam dimensions 0.2*0.3*11 with reinforcement concrete ratio 1:2:4 by using 4 bars Ø 12mm  and steel barsØ  6mm 20cm c/c .
	ML
	11
	
	

	27
	Provide materials & cast reinforcement concrete slap  dimensions 3*2.5*.15 with reinforcement concrete ratio 1:2:4 steel bars  mesh Ø12mm  at 15cm c/c  both ways, curing for at least 7 days, 3 tims /day latrine hole should be on to the slap diameter 15cm according to   tecknical drawings, install on the slab 1 manhole 50*50cm by casting manhole frame, according to tecknical drawing.
	M³
	1.1
	
	

	28
	Provide and build 1 (one) brick wall total height 3m of first class ordinary burnt red clay bricks in c/s  use cement mortar 1:6 with proper curing for three days
	M²
	29
	
	

	29
	Provide and construct the  roof by metallic corrugated sheet 0.35mm thickness using the nesessary and required stainless steel bolts with all  it's accessories including the rubber supported with 4*8cm steel pipes including all the necessary welding work as per the jop specification and the required paints [one face anti-rustpaints+two faces steel paints].
	M²
	5
	
	

	30
	Provide and install 2 doors 0.8**2m manufactured of Heavy 3*6 cm  pipes and heavy metallic sheet 0.8 mm  including all necessary welding work  and it's accessories (handle,lock,fiberglass,...) as well as  the required paints (one face anti-rust paint + two faces oily paints),as per the detailes and drawings .
	no
	2
	
	

	31
	provide & fix ligt windows size 30*30 cm made of heavy iron angle 3/4 inch and steel fine mesh with painting[one face anti-rustpains + twofaces steel paints].
	no
	2
	
	

	32
	provide 20mm sand cement mortar 1:6 for external and internal plastering of the walls
	M²
	63
	
	

	33
	painting  for Internal & external finishing  of the walls (three faces use bombastic)with CRS Logo
	M²
	63
	
	

	34
	casting reinforced concrete 0.2 width *1.5 length * 0.12m thickness by using 4 Ø 12mm steel bars
	pcs
	2
	
	

	35
	casting concrete manhole cover 70*70*15cm by using steel reinforcement mesh 12 mm bars both ways c/c
	pcs
	1
	
	

	36
	Provide materials and build complete separation wall with finishing height 2 m as( T shape) from red bricks no 1 by cement mortar mix (1:6)  1 bricks thickness after excavating strip foundation fore  the T shape [5m length,40cm depth , and 40 cm width ], plastering , painting as well as plan concreate and ramp with handrail for both side according  to the  Satisfaction  of the engineer 
	 L.s
	1
	
	

	37
	provide and install metallic gender sign with dimension 30*30 cm
	pcs
	2
	
	

	38
	provide and install local ceramic seats
	pcs
	2
	
	

	39
	provide and install one PVC ventilation pipe 4 inch 
	pcs
	2
	
	

	Waste Management Abojabra:

	40
	Provide 20mm sand cement mortar1:6 for external and internal plastering of the walls.
	M²
	15
	
	

	41
	Provide and install  doors 60*60 cm manufactured of Heavy angle 2 inch and heavy metallic sheet 0.8 mm  including all necessary welding work  and it's accessories (handle, lock, fiberglass,...) as well as  the required paints (one face anti-rust paint + two faces oily paints)
	NO
	2
	
	

	42
	provide and install Expand inside of the incinerator 
	M²
	4
	
	

	43
	 external finishing painting  for the walls (three faces use bombastic)).
	M²
	15
	
	

	44
	Excavation, construction, and commissioning of two simple disposal pits, comprising one ash disposal pit with internal dimensions of 1.00 × 1.00 × 1.50 m, and one disposal pit for sharps and non-combustible waste with internal dimensions of 1.00 × 1.00 × 2.00 m as will as  provide and construct pit cover using local materials (timber , wooden poles ,  plastic sheeting and compacted soil) including all material , labor , fixing and all associated works 
	job
	1
	
	

	45
	Provide material  and fix  in position Metal Boundary Fence around the incinerator  composed of vertical Angle 2 inch 3mm thickness  2.5 m length, Penetrate 50 cm and fix by concrete base 30 cm X 30 cm X 40 cm each 2 m C/C  ,the horizontal elements tension wires 4 rows to fix chain-link mesh 50 mm X 50 mm (Gabyan ) to the  Satisfaction  of the engineer 
	ML
	7
	
	

	46
	Provide materials & fabricate Door size 1*2 m should be made from steel pipe of 4*8 cm for external door frame, the internal work from 3*6 cm pipe  every 10 cm . The door should be with full accessories (handle,locks,joints,...)  and the required paints (one face anti-rust paint + two faces steel paints) . the Door fix properly with good suport according  to the  Satisfaction  of the engineer .
	NO
	1
	
	

	Renovation of rooms Abojabra:


	47
	 dismantle of the existing wall (3*2m) and Provide materials & fabricate the main gate size 3 *2.2 m should be made from steel pipe of 4*8 cm  thichness 1mm for external door frame, the internal work from 3*6 cm pipe  every 10 cm . The door should be with full accessories (handle,locks,joints,...)  and the required paints (one face anti-rust paint + two faces steel paints) fix properly on two column from red bricks,plain concreate ( 3 length , 1.5 wide , .15 thickness), use cement morter  according  to the  Satisfaction  of the engineer .
	NO 
	1
	
	

	48
	Modification of door and window openings by relocating and installing the door at the existing window location and relocating and installing the window at the existing door location, including all necessary demolition and alteration works, closing the remaining portion of the door opening with brickwork and cement mortar, and making good all finishes to complete the work  according  to the  Satisfaction  of the engineer .
	job
	1
	
	

	49
	inspect and repair leakage points in the existing corrugated zinc of room(4*4m) including sealing joints , overlaps , fixing points and all necessary  works to prevent rainwater penetration complete as directed by the engineer   
	job
	1
	
	

	50
	external finishing painting  for the walls (three faces use pomaatic))with CRS Logo based on the supervisor's instructions.
	M²
	268
	
	

	51
	supply and install suspended ceiling to replace damaged sections caused by water leakage , including removal of damaged ceiling panels , disposal of debris , provision of all accessories , framing  members , and fixing materials , replacement area approximately 8M² complete as directed by the engineer
	M²
	8
	
	

	Water Connection Abojabra:

	52
	Provide  Polyethylene 1'' high quality including all necessary fittings  and connect it on the end out let of (tiga)  and excavation and backfill of the trench with well compaction. 
	ML
	60
	
	

	53
	provide material and construct base for water storge 1500 litter using red bricks and sand / cement mortar in size 2.5 m x 2.5 m and height 1.5 m and cover at top by reinforced concrete thickness 12 cm and construct steps leader  with hand rails as instructed by engineer
	job
	1
	
	

	54
	provide and install water storge 1500 liters  horizontal ( tiga ) with in let , out let from PPR 1 inch 
	job
	1
	
	

	55
	Supply and installation of 2 taps 3/4 inch at latrine  with PPR and , including all necessary fittings ( valves, elbows, sockets ,......) , accessories, and connection to the existing water supply line. and everything necessary for the complete execution of the work.
	NO
	2
	
	

	56
	Supply and installation of a 1-inch water tap fixed to the boundary wall with PPR  for PH use , including all necessary fittings ( valves, elbows, sockets ,......), accessories, and connection to the existing water supply line. The item shall also include the construction of a 50 × 50 cm brick masonry basin around the tap, complete with plastering and finishing, 
	NO
	1
	
	

	Total

	






























ATTACHED (2)
Lot#2 Bahralarab SC

	East Dar fur - Bahralarab SC 
Bill of Quantity for Repair Bahar Alarab SC rooms, repair the existing latrine, repair the medical waste incinerator, connect to a water supply build a kitchen with local material, Zink, Rehabilitation of west management


	
		Fence & Renovation rooms Bahralarab:

	1
	Provide and construct the Project sign-board ,fabricated from 4" circular steel pipe as stands height 1.5, casted by concrete with required depth (50cm) , well welded with heavy sheets 1mm thickness, 150cm*100cm for width and height respectively. All the components  should be painted (one face anti-rust paint + two faces steel paints). All the Project informations should be written on the sign-board based on the supervisor's instructions.
	L.S
	1
	
	

	2
	 maintenance of the existing  Fence  the maintenance including   provide and fixing American zinc  hight 1.7m ,provide and fix  horizontal elements tension square pipe 8*4  1mm thickness 3 rows to fix American zinc  using the necessary welding and required stainless steel bolts  and  paints (one face anti-rust paint + two faces steel paints) according  to the  Satisfaction  of the engineer
	ML
	55
	
	

	3
	Provide material  and construct Metalic   Fence composed of American zinc , vertical square pipe 4*8 cm  2.5 m hight, Penetrate 50 cm and fix by concrete base 40 cm X 40 cm X 40 cm each 2 m C/C ,the horizontal elements tension square pipe 3*6  1mm thickness 3 rows to fix American zinc  using the necessary welding and required stainless steel bolts  and  paints (one face anti-rust paint + two faces steel paints) according  to the  Satisfaction  of the engineer
	ML
	31
	
	

	4
	maintenance of 3 doors and the maintenance including  Sliding bolt, repainting  , complete in all respects  according  to the  Satisfaction  of the engineer .
	NO
	3
	
	

	5
	maintenance of 4 windows and the maintenance including  Sliding bolt , repainting , complete in all respects  according  to the  Satisfaction  of the engineer .
	NO
	4
	
	

	6
	maintenance of 10 windows and the maintenance including  repainting , complete in all respects  according  to the  Satisfaction  of the engineer .
	NO
	10
	
	

	7
	Inspection and re-fixing of floor ceramic tiles in six rooms, including white cement grouting, and supply and installation of 4 m² of new ceramic floor tiles, complete in all respects.
	job
	1
	
	

	8
	renovation of some cracks at the wall of building  use cement mortar mix (1:4) according  to the  Satisfaction  of the engineer 
	M²
	10
	
	

	9
	inspect and repair leakage points in the existing corrugated zinc of 6 room (4*4m) including sealing joints , overlaps , fixing points and all necessary  works to prevent rainwater penetration complete as directed by the engineer   


	job
	1
	
	

	10
	external and internal finishing painting  for the walls (three faces use pomaatic))with CRS Logo based on the supervisor's instructions.
	M²
	391
	
	

	11
	Dismaintal existing wall (4*2m) and build wall  1.5  brick wall in the main building   hight  2 m  .Should use first class ordinary burnt red clay brick in c/s  , mortar 1:6 with proper curing for three days. As well as plastering and finishing painting 
	M²
	8
	
	

	12
	 Cover the internal areas( partition)  from elevation 2.8 m hight and 2.4 length  , in the main building   , by heavy American zinc, the horizontal elements tension square pipe 3*6  1mm thickness 3 rows to fix American zinc including all the necessary items and work[connections, steel nails] to be fixed properly
	M²
	7.5
	
	

	13
	 provide and install Heat  insulator for  American zinc  sheets according  to the  Satisfaction  of the engineer
	M²
	15
	
	

	14
	Provide and install  doors 1*2.2m manufactured of Heavy 3*6 cm  pipes and heavy metallic sheet 0.8 mm  including all necessary welding work  and it's accessories (handle,lock,fiberglass,...) as well as  the required paints (one face anti-rust paint + two faces oily paints),
	NO
	1
	
	

	15
	construction of local kitchen ( karank)  with dimention (  4*6*3m wide ,lenght,hight) using local materials wooden poles(sha,ab) , bamboo stick (cane) , grass mats (Sharghani) , bamboo sheet (haseer ) and all necessary local materials for complete construction including fabrication and installation of one door made from local materials ( bamboo).roof covering with heavy plastic sheet  to prevent rainwater penetration , complete with all labor ,tools transportation , fixing and every thing required for a fully completed kitchen according  to the  Satisfaction  of the engineer .
	Job
	1
	
	

	Latrine Maintenance Bahralarab:


	16
	Modification of 4 door(2*.8m)  and 4window(0.3*0.3) openings by relocating and installing the doors at the existing windows location and relocating and installing the windows at the existing doors location, including all necessary demolition and alteration works, closing the remaining portion of the doors opening with brickwork and cement mortar, and making good all finishes to complete the work  according  to the  Satisfaction  of the engineer .

	job
	1
	
	

	17
	provide and construct ramp  ( steps  , slop  for people with disability) for  latrine entrance with dimensions(1.5*5m)   use red bricks, cement mortar  and plain concreate  including all the finishing according to the engineer instructions 
	job
	1
	
	

	18
	Internal and external finishing painting  for the walls (three faces use bombastic)) 

	M²
	32
	
	

	Waste Management Bahralarab:


	19
	renovation of some cracks at the wall of incinerator use cement mortar mix(1:4) according  to the  Satisfaction  of the engineer .
	M²
	2
	
	

	20
	Provide and install  doors 60*60 cm manufactured of Heavy angle 2 inch and heavy metallic sheet 0.8 mm  including all necessary welding work  and it's accessories (handle, lock,...) as well as  the required paints (one face anti-rust paint + two faces oily paints)
	NO
	2
	
	

	21
	provide and install Exbanda inside of the incinerator 
	M²
	4
	
	

	22
	 external finishing painting  for the walls (three faces use pomaatic)).
	M²
	13
	
	

	23
	Excavation, construction, and commissioning of two simple disposal pits, comprising one ash disposal pit with internal dimensions of 1.00 × 1.00 × 1.50 m, and one disposal pit for sharps and non-combustible waste with internal dimensions of 1.00 × 1.00 × 2.00 m as will as  provide and construct pit cover using local materials (timber , wooden poles ,  plastic sheeting and compacted soil) including all material , labor , fixing and all associated works 
	job
	1
	
	

	24
	Provide material  and fix  in position Metal Boundary Fence around the incinerator  composed of vertical Angle 2 inch 3mm thickness  2.5 m length, Penetrate 50 cm and fix by concrete base 30 cm X 30 cm X 40 cm each 2 m C/C  ,the horizontal elements tension wires 4 rows to fix chain-link mesh 50 mm X 50 mm (Gabyan ) to the  Satisfaction  of the engineer 
	ML
	7
	
	

	25
	Provide materials & fabricate Door size 1*2 m should be made from steel pipe of 4*8 cm for external door frame, the internal work from 3*6 cm pipe  every 10 cm . The door should be with full accessories (handle, locks, joints,...)  and the required paints (one face anti-rust paint + two faces steel paints) . the Door fix properly with good support according  to the  Satisfaction  of the engineer .
	NO
	1
	
	

	Water Connection Bahralarab:

	26
	Provide  Polyethylene 1'' high quality including all necessary fittings  and connect it on the end out let of (tiga)  extended to  latrine and  hand washing facility  and exavation and backfill of the trench with well compaction. 
	ML
	60
	
	

	27
	Supply and installation of 4 taps 3/4 inch at latrine  with PPR and , including all necessary fittings ( valves, elbows, sokets ,......) , accessories, and connection to the existing water supply line. and everything necessary for the complete execution of the work.
	NO
	4
	
	

	28
	Supply and installation of a 1-inch water tap fixed to the boundary wall with PPR  for PH use , including all necessary fittings ( valves, elbows, sokets ,......), accessories, and connection to the existing water supply line. The item shall also include the construction of a 50 × 50 cm brick masonry basin around the tap, complete with plastering and finishing, 
	job
	1
	
	

	Total
	















	


ATTACHED (3)
Lot#3 Sheria SC

	East Dar fur      -     Sheria SC 
Bill Of Quantity for repair Sheria SC rooms, connect to a water supply, construct a kitchen with local materials, repair the existing latrine, install a solar power system. Rehabilitation of west management

	
		Maintenance of rooms Sheria:

	No
	Description
	Unit
	Qty
	U. Price USD
	Total USD

	1
	maintenance of  door  the maintenance including   new lock  and it's accessories  as according  to the  Satisfaction  of the engineer .
	NO
	1
	
	

	2
	Provide and build 1 (one) brick wall as partition with total height 2.8m of first class ordinary burnt red clay bricks in c/s  use cement mortar 1:6 with proper curing for three days including  plastering and finishing painting
	M²
	11
	
	

	3
	Supply and install 6 mm frosted glass for 20 windows, including fanlights, complete with all necessary accessories and fixing, as per specifications.
	M²
	20
	 
	 

	4
	Provide and install  doors 120*2.2m manufactured of Heavy 3*6 cm  pipes and heavy metallic sheet 0.8 mm  including all necessary welding work  and it's accessories (handle,lock,fiberglass,...) as well as  the required paints (one face anti-rust paint + two faces oily paints),as per the detailes and drawings .
	NO
	1
	
	

	5
	external and internal finishing painting  for the walls (three faces use pomaatic))with CRS Logo based on the supervisor's instructions.
	M²
	383
	
	

	Construction of Fence:

	6
	Excavations of  holes size 40cm*40cm and depth 40cm, the price includes excavation , and transportation of excavated material to .approved dump area according to the supervaisor 
	NO
	59
	
	

	7
	Provide and install of Angle 2.5 inch thickness 5 mm each 2 m total Angle height 2.5 m with support each 4m, should be casted by 40 cm by plain concreted, the price included all material and workmanship & tools... etc,  in accordance to specification and supervisor instruction.
	NO
	59
	
	

	8
	provide and install   steel bar Ø 10mm , at three elevation (3 lines) from bottom to the top of the fence to support the metallic wire net later  , good installation must be done by welding , the price included all material and workmanship & tools etc, ,needed  ,in accordance to specification and supervisor instruction.
	ML
	468
	
	

	9
	provide and install metallic wire net (chain-lock) for the fence, thickness 3 mm (5 cm*5 cm) , fence height 2 m
	M²
	234
	
	

	10
	Provide materials & fabricate Door size 3*2.2 m should be made from steel pipe of 5*10 cm for external door frame, the internal work from 3*6 cm pipe  every 10 cm . The door should be with full accessories (handle,locks,joints,...)  and the required paints (one face anti-rust paint + two faces steel paints) . the door should be fixed on colummn from red bricks size(.8*.8*2.5 m) use cement mortar mix 1:6
	NO
	1
	
	

	11
	construction of local kitchen ( karank)  with dimention (  4*6*3m wide ,lenght,hight) using local materials wooden poles(sha,ab) , bamboo stick (cane) , grass mats (Sharghani) , bamboo sheet (haseer ) and all necessary local materials for complete construction including fabrication and installation of one door made from local materials ( bamboo).roof covering with heavy plastic sheet  to prevent rainwater penetration , complete with all labor ,tools transportation , fixing and every thing required for afully completed kitchen according  to the  Satisfaction  of the engineer .
	Job
	1
	
	

	12
	Provide and construct the Project sign-board ,fabricated from 4" circular steel pipe as stands height 1.5, casted by concrete with required depth (50cm) , well welded with heavy sheets 1mm thickness, 150cm*100cm for width and height respectively. All the components  should be painted (one face anti-rust paint + two faces steel paints). All the Project information should be written on the sign-board based on the supervisor's instructions.
	L S
	1
	
	

	Latrine Sheria:

	13
	Provide and install 3 doors( 0.6*1.8m )manufactured of Heavy 3*6 cm  pipes and heavy metallic sheet 0.8 mm  including all necessary welding work  and it's accessories (handle, lock, fiberglass,...) as well as  the required paints (one face anti-rust paint + two faces oily paints),as per the details and drawings .
	NO
	3
	
	

	14
	renovation of some cracks at the wall of latrine  use cement mortar Mix(1:4)  according  to the  Satisfaction  of the engineer .
	M²
	1
	
	

	15
	provide and install local ceramic seats
	NO
	3
	
	

	16
	provide and construct ramp  ( steps  , slop  for people with disability) for latrine entrance (4*1m)  use red bricks, cement mortar mix(1:6)  and plain concreate  including all the finishing according to the engineer instructions 
	job
	1
	
	

	17
	Internal and external finishing painting  for the walls (three faces use Bombastic)) 

	M²
	72
	
	

	Water Connection Sheria:

	18
	Provide  Polyethylene 1'' high quality including all necessary fittings  and connect it on the existing  main water supply line  and the end out let of (tiga)  and exavation and backfill of the trench with well compaction. 
	ML
	20
	
	

	19
	provide material and costruct base for water storge 1500 litter using red bricks and sand / cement morter in size 2.5 m x 2.5 m and height 1.5 m and cover at top by reinforced concrate thickness 12 cm and costruct steps leader  with hand rails as instructed by engineer
	job
	1
	
	

	20
	provide and install water storge 1500 liters  horizantal ( tiga ) with in let , out let from PPR 1 inch 
	job
	1
	
	

	21
	Supply and installation of 3 taps 3/4 inch at latrine  with PPR and , including all necessary fittings ( valves, elbows, sokets ,......) , accessories, and connection to the existing water supply line. and everything necessary for the complete execution of the work.
	NO
	3
	
	

	22
	Supply and installation of a 1-inch water tap fixed to the boundary wall with PPR  for PH use , including all necessary fittings ( valves, elbows, sockets ,......), accessories, and connection to the existing water supply line. The item shall also include the construction of a 50 × 50 cm brick masonry basin around the tap, complete with plastering and finishing, 
	NO
	1
	
	

	Waste Management Sheria:

	23
	Excavation, construction, and commissioning of two simple disposal pits, comprising one ash disposal pit with internal dimensions of 1.00 × 1.00 × 1.50 m, and one disposal pit for sharps and non-combustible waste with internal dimensions of 1.00 × 1.00 × 2.00 m as will as  provide and construct pit cover using local materials (timber , wooden poles ,  plastic sheeting and compacted soil) including all material , labor , fixing and all associated works 
	job
	1
	
	

	24
	Provide material  and fix  in position Metal Boundary Fence around the incinerator  composed of vertical Angle 2 inch 3mm thickness  2.5 m length, Penetrate 50 cm and fix by concrete base 30 cm X 30 cm X 40 cm each 2 m C/C  ,the horizontal elements tension wires 4 rows to fix chain-link mesh 50 mm X 50 mm (Gabyan ) to the  Satisfaction  of the engineer 
	ML
	15
	
	

	25
	Provide materials & fabricate Door size 1*2 m should be made from steel pipe of 4*8 cm for external door frame, the internal work from 3*6 cm pipe every 10 cm . The door should be with full accessories (handle, locks, joints,...)  and the required paints (one face anti-rust paint + two faces steel paints) . the Door fix properly with good support according  to the Satisfaction  of the engineer .

	NO
	1
	
	

	Total
	



ATTACHED (4)
Lot#4 Solar System Abojabra, Bahralarab and Sheria


	Abojabra Solar:

	 No
	 Item description
	Unit
	Qty
	U.Price USD
	Total USD

	1
	 provide Solar panels equal to  (Monocrystalline) Jinko 550Watt 
	Pcs
	8
	
	

	2
	 provide 5KW/48V hybrid solar inverter , compatible with  lithum Batteries
	Pcs
	1
	
	

	3
	supply of lithum Battery 48V, 5kWh capacity  complete with all accessories
	pcs
	1
	
	

	4
	supply and installation of 6mm^2 solar DC cable , UV resistant , complete with MC4 connectors and accessories 
	M
	25
	
	

	5
	supply and installation of 16mm^2 flexible copper battery cable  , complete with cable lugs  and accessories .
	M
	2
	
	

	6
	 supply suitable Solar circuit breaker  AC anb DC
	Pcs
	2
	
	

	7
	provide terank 2 cm 
	Pcs
	40
	
	

	8
	Solar stand made by heavy 2 inch iron angle to hold 8 solar panels
	Pcs
	1
	
	

	9
	supply and installation of orient ceiling fan indian made ,56-inch sweed , complete with downrod  , regulator , mounting Accessories  
	NO
	6
	
	

	10
	provide lamp 12 W
	NO
	30
	
	

	11
	Switch of lamp
	NO
	30
	
	

	12
	seat of lamp
	NO
	30
	
	

	13
	Balak 13 Ambir
	NO
	15
	
	

	14
	Cable 2.5 mm for Internal connection Al-fanar
	roll
	4
	
	

	15
	Cable 1.5 mm for Internal connection Al-fanar
	roll
	2
	
	

	16
	Labor cost for installation of solar system and connection with the Lamp,Fans&plugs the price including transportation of materials , the exavation and casting  of footing and weilding and whatever it take to working 
	Job
	1
	
	

	Bahralarab Solar:

	17
	 provide Solar panels equal to  (Monocrystalline) Jinko 550Watt 
	Pcs
	8
	
	

	18
	 provide 5KW/48V hybrid solar inverter , compatible with  lithum Batteries
	Pcs
	1
	
	

	19
	supply of lithum Battery 48V, 5kWh capacity  complete with all accessories
	pcs
	1
	
	

	20
	supply and installation of 6mm^2 solar DC cable , UV resistant , complete with MC4 connectors and accessories .
	M
	25
	
	

	21
	supply and installation of 16mm^2 flexible copper battery cable  , complete with cable lugs  and accessories .
	M
	2
	
	

	22
	 supply suitable Solar circuit breaker  AC anb DC
	Pcs
	2
	
	

	23
	provide terank 2 cm 
	Pcs
	40
	
	

	24
	Solar stand made by heavy 2 inch iron angle to hold 8 solar panels
	Pcs
	1
	
	

	25
	supply and installation of orient ceiling fan indian made ,56-inch sweed , complete with downrod  , regulator , mounting Accessories  
	NO
	6
	
	

	26
	provide lamp 12 W
	NO
	30
	
	

	27
	Switch of lamp
	NO
	30
	
	

	28
	seat of lamp
	NO
	30
	
	

	29
	Balak 13 Ambir
	NO
	15
	
	

	30
	Cable 2.5 mm for Internal connection Al-fanar
	roll
	4
	
	

	31
	Cable 1.5 mm for Internal connection Al-fanar
	roll
	2
	
	

	32
	Labor cost for installation of solar system and connection with the Lamp,Fans&plugs the price including transportation of materials , the exavation and casting  of footing and weilding and whatever it take to working 
	Job
	1
	
	

	Sheria Solar:

	33
	 provide Solar panels equal to  (Monocrystalline) Jinko 550Watt 
	Pcs
	8
	
	

	34
	 provide 5KW/48V hybrid solar inverter , compatible with  lithum Batteries
	Pcs
	1
	
	

	35
	supply of lithum Battery 48V, 5kWh capacity  complete with all accessories
	pcs
	1
	
	

	36
	supply and installation of 6mm^2 solar DC cable , UV resistant , complete with MC4 connectors and accessories .
	M
	25
	
	

	37
	supply and installation of 16mm^2 flexible copper battery cable  , complete with cable lugs  and accessories .
	M
	2
	
	

	38
	 supply suitable Solar circuit breaker  AC anb DC
	Pcs
	2
	
	

	39
	provide terank 2 cm 
	Pcs
	40
	
	

	40
	Solar stand made by heavy 2 inch iron angle to hold 8 solar panels
	Pcs
	1
	
	

	41
	supply and installation of orient ceiling fan indian made ,56-inch sweed , complete with downrod  , regulator , mounting Accessories  
	NO
	6
	
	

	42
	provide lamp 12 W
	NO
	30
	
	

	43
	Switch of lamp
	NO
	30
	
	

	44
	seat of lamp
	NO
	30
	
	

	45
	Balak 13 Ambir
	NO
	15
	
	

	46
	Cable 2.5 mm for Internal connection Al-fanar
	roll
	4
	
	

	47
	Cable 1.5 mm for Internal connection Al-fanar
	roll
	2
	
	

	48
	Labor cost for installation of solar system and connection with the Lamp,Fans&plugs the price including transportation of materials , the exavation and casting  of footing and weilding and whatever it take to working 
	Job
	1
	
	

	
	
	
	
	
	










	
	


ATTACHED (5)
Scope of Work (SoW) for Rehabilitation of Three SCs in Abojabra, Abomatarig and Sheria East Darfur
Catholic Relief Services (CRS) intends to rehabilitate selected SCs facilities located in Abojabra, Abomatarig and Sheria East Darfur State, Sudan. The rehabilitation works aim to restore and improve the functionality, safety, and quality of healthcare infrastructure to ensure the delivery of essential health services in accordance with Ministry of Health standards and humanitarian best practices. CRS infrastructure projects typically prioritize safety, functional facilities with reliable water, sanitation, and quality construction.
The contractor shall provide all labor, materials, equipment, tools, transportation, supervision, and technical services necessary to complete the rehabilitation works.
The contractor’s responsibilities:
The specific tasks of the contractor under this scope of work should be implemented under direct supervision and instruction of CRS field staff, and each completed stage of the work should be accepted and approved by CRS field staff, and the contractor should implement and complete any required repair or amendment before starting the next stage, also contractor should be responsible to the following:
1- Materials
· All materials shall be new, unused, and approved quality by Project Engineer
· The materials shall be complied with the technical specifications and applicable Sudanese or internationally recognized standards
· Samples shall be submitted for approval by Project Engineer before procurement where required.


2- Quality Control
The contractor shall:
· Implement a quality control system throughout the rehabilitation period.
· Conduct all required inspections and testing (if need).
· Correct defective work at no additional cost
· Maintain records of inspections and test results.
3- Health, Safety, and Environmental (HSE) Requirements
The contractor shall
· Comply with national occupational health and safety regulations and CRS safety requirements.
· Provide appropriate personal protective equipment (PPE) to all workers
· Maintain first did facilities on site.
· Prevent environmental pollution.
· Control dust, noise, and rehabilitation waste.
· Protect patients, health workers, and visitors during rehabilitation activities.
4- Environmental and Social Safeguards
The contractor shall:
· Minimize disruption to health services.
· Ensure safe access for patients and staff.
· Prevent child labor and forced labor.
· Prevent gender-based violence, sexual exploitation, abuse, and harassment (GBV/SEAH).
· Respect local communities and cultural practices.
· Adhere to CRS safeguarding and code of conduct requirement.
5- Schedule
· Commence works immediately upon receipt of the notice proceed.
· Complete all work within the period specified in the contract.
· Submit a detailed work program showing activity sequencing, milestones and completion dates.
       6- Inspection and Supervision
        The works shall be supervised by CRS and/or designated Engineer. The contractor shall:
· Provide unrestricted access to the site.
· Cooperate during inspections.
· Rectify defects identified during inspections within the specified timeframe.
        7- Testing and Commissioning
           The contractor shall perform all required testing and commissioning of electrical,     
       plumbing, and other building systems before handing over.
         8- Handover
             Upon completion, the contractor shall:
· Thoroughly clean the site 
· Remove temporary work and unused materials
· Submit as-built drawings where applicable.
· Provide warranties and operation manual for installed equipment.
· Remedy all defects identified during the Defect Liability period.
         9- Deliverables 
             The contractor shall submit:
· Work program and implementation schedule.
· Materials submittals and approvals.
· Quality assurance documentation.
· Weekly or biweekly progress reports.
· Inspection and testing records.
· Completion report.
· As-built drawings (where applicable).
· Defect liability commitments.

         10- Applicable Documents
             The work shall be executed in accordance with:
· Approval architectural, structural, electrical, and plumbing drawings.
· Technical Specifications.
· Bill of Quantities (BoQ).
· Contract Conditions.
· CRS construction standards and safeguarding requirements.
· Applicable Sudanese Building codes and Ministry of Health requirements.

	        
Bidder’s (Company) Name: ________________

Authorized Person Full Name: _____________
Title (Position):	_________________________

Signature and Company Official Stamp:	_____

Date: ____________________

	
اسم مقدم العرض (الشركة)___________________

الاسم الكامل للشخص المفوض: _________________ 

اللقب (المنصب): ___________________________

التوقيع وختم الشركة الرسمي: _______________

التاريخ:___________________________




