

**BOQ for construction one incinerator**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **item** | **SPACIFICATIOPNS** | **UNIT** | **QUT** | **Unit Price** | **Total Amount** |
| **1** | Cast plain concrete 5cm 2×2 under platform | M2 | 4 |  |  |
| **2** | Cast reinforced concrete 10cm thick - 2×2m as incinerator platform. | M2 | 4 |  |  |
| **3** | Building ½ brick 2layer wall by thermal brick) & thermal cement mortar for 1½×1½m incinerator outer dimension.1.1m high | M2 | 7 |  |  |
| **4** | Installation of ash sieve by 3 leaner bar with 2 cm space. | M2 | 1.8 |  |  |
| **5** | Cast reinforced concrete 7cm thick for incinerator cover 10cm thickness | M2 | 2.25 |  |  |
| **6** | installation of 3 inch D circular metal ventilation pipe (3m ) | PCS | 1 |  |  |
| **7** | installation of metal high level plate cover size 50x50cm framed by angle 2 inch | PSC | 3 |  |  |
| **8** | Installation of 3×3m fence using circular 3 inch D petal pipe and barbed mesh 2.5mm. The height is 2m.The price contains installation of door. | M l | 12 |  |  |
|  | **Total Cost** | | |  | |