**BOQ for construction of latrine that have two seats and two doors**

**Location: BLNS**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Item** | **SPACIFICATIOPNS** | **UNIT** | **QUT** | **Unit Price** | **Total Amount** |
| **1** | Excavation for septic tank 3\*3\*2.5 | M3 | 22.5 |  |  |
| **2** | Excavation for strip foundation 50\*50cm for privacy wall | M l | 6.5 |  |  |
| **3** | Cast plain concrete 5cm for septic tank | M3 | 0.5 |  |  |
| **4** | Building 1.5brick wall by red brick class (1) & cement mortar 1:8 for privacy wall foundation | M2 | 5.5 |  |  |
| **5** | Cast reinforced concrete 10cm thick for septic tank | M3 | 0.9 |  |  |
| **6** | Cast grade beam 20\*20cm for privacy wall & Cast lintel tie beam 20\*10cm | M3 | 0.4 |  |  |
| **7** | Cast reinforced concrete 12.5cm thick for septic tank cover | M3 | 1.1 |  |  |
| **8** | Building 1.5 brick wall by red brick class (1) & cement mortar 1:8 until 20cm above ground level for septic tank | M2 | 36 |  |  |
| **9** | Building 1 brick wall with cement mortor1;8 for privacy &latrine wall contains parapet | M2 | 36 |  |  |
| **10** | Supply and fix the roof by zinc sheet 0.35mm using painted metal pipes 3× 6 (1 inch ) as purlin. | M2 | 9 |  |  |
| **11** | Make Cement plaster for inside and outside of All latrine wall , mixed 1:8 | M2 | 115 |  |  |
| **12** | Paint for inside and outside of All latrine walls. | M2 | 115 |  |  |
| **13** | Installation of Ventilations Pipe PVC 4 inches length 3m | NO | 1 |  |  |
| **14** | Installation of door with dimensions (70x190 cm) meters of steel plate & pipes 3×6. | Door | 2 |  |  |
| **15** | Installation of Steel high level Windows size 40x40cm | Window | 2 |  |  |
| **16** | Manhole cover |  | 1 |  |  |
| **17** | Installation of Marble toilet seat | seat | 2 |  |  |
| **18** | Construction of ramp for access to disable persons to the door | No | 2 |  |  |
| **19** | Construction of hand washing facility have three copper tabs and connection of water to hand washing facility | HWF | 1 |  |  |
| **20** | Drawing colorful Handwashing and latrine use(IEC) messages communication at the wall of the latrine as per Engineers instruction | No | 2 |  |  |
|  | **Total Cost** | | |  | |