

**BoQ for Slab and Beam for HH latrine**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **No** | **Description** | **Unit** | **Quantity** | **Unit price** | **Total price** |
| 1 | Provide materials & make Reinforced concrete Slab size 80\*80cm and 6cm thickness using mix ratio **1:2:4** Using iron bar 10mm (3 linya) 8 pcs 75cm long, tied with bending wire as per attached drawing. | PCs | 1150 |  |  |
| 2 | Provide materials & make Reinforced concrete Beam size 160\*15cm and 8cm thickness using mix **1:2:4** using iron bar 10mm (3 linya) 2 pcs. | PCs | 2300 |  |  |
|  | **Total Cost** |  |

Amount in Word: -------------------------------------------------------------------------------------

------------------------------------------------------------------------------------------------------------

Company name: ---------------------------------------------------------------------------------------

Duration of time to complete: -----------------------------------------------------------------------

Date: ----------------------- Signature: -------------------------------- Stamp :------------------