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Amendment No. 3
Dear Sirs,
This Amendment No. 3 shall form an integral part of the Bidding Document. It supersedes the corresponding provisions of the Bidding Document, Amendments Nos. 1 and 2, and the Pre-Bid Clarification to Queries only to the extent expressly stated below. All other provisions remain unchanged.
	Item No. 1
	Extension of Bid Submission and Opening Deadline
In the Specific Procurement Notice – Request for Bids, paragraph 6, and Section II – Bid Data Sheet (BDS), ITB 22.1, and Item No. 1 of Amendment No. 2, please amend the Bid submission deadline from:
“27th August 2026 at 12:00 PM Sudan Time”
to:
“13th September 2026 at 12:00 PM Sudan Time.”
Similarly, in the Specific Procurement Notice – Request for Bids, paragraph 6, and Section II – Bid Data Sheet (BDS), ITB 25.1, please amend the Bid opening date and time from:
“27th August 2026 at 12:00 PM Sudan Time”
to:
“13th September 2026 at 12:00 PM Sudan Time.”

	Item No. 2
	Revision of Equipment Names and Motor Requirements
In the Specific Procurement Notice, Section VII – Schedule of Requirements, Summary of Technical Specifications, applicable Bills of Quantities (BOQs), and related references throughout the Bidding Document, please adopt the following equipment names and motor ratings:
	Item No.
	Equipment Description
	Required Motor Rating
	Quantity

	1
	Grain Cleaning System
	8 kW
	6 sets

	2
	Grain Skin Peeling / Removing Machine
	3 kW
	6 sets

	3
	Locally Fabricated Oil Press
	11 kW
	6 sets

	4
	Grain Miller
	15 kW
	6 sets


The above descriptions supersede the equipment naming arrangement under Item No. 2 of Amendment No. 1. The 3 kW machine shall be the Grain Skin Peeling/Removing Machine; a separate Spice Mills Grinder is not required.
Corresponding references in the installation, testing, commissioning and motor-drive descriptions shall be read as referring to the applicable equipment listed above.

	Item No. 3
	Removal of Specified Production Capacities 
In Section VII – Schedule of Requirements, Summary of Technical Specifications and the applicable equipment BOQs, please delete the specified numerical production/output capacities as follows:
	Equipment
	Requirement Deleted

	8 kW Grain Cleaning Machine
	500 kg/hour

	3 kW machine, now designated Grain Skin Peeling/ Removing machine
	400-500 kg/hour

	Oil Press
	150kg/hour

	Grain Miller
	150kg/hour


In the Summary of Technical Specifications, please delete the words “processing capacity” from the requirements for the four machines.
The motor ratings specified under Item No. 2 of this Amendment remain mandatory. Removal of the numerical output capacities does not remove the requirements for suitability for the stated processing functions, installation, functional testing, successful trial operation and commissioning.
Clarification Q6 of the Pre-Bid Clarification to Queries shall be read accordingly.

	Item No. 4
	Locally Fabricated Oil Press
In Section VII – Schedule of Requirements, BOQ for the Solar-Powered Oil Press System, Item No. 1 – Oil Press Equipment, please replace the existing equipment specification with:
“11 kW locally fabricated multi-purpose oil press, suitable for processing groundnut, sesame, sunflower and similar oilseeds.”
The oil press shall be locally fabricated. An imported oil press shall not satisfy this requirement.
The explicit cold-press requirement introduced under Item No. 3 of Amendment No. 1 and reflected in Clarification Q2 is deleted. No separate requirement concerning soaked seeds is introduced.
The attached oil storage tank remains required, with a total quantity of six (6) tanks, one for each oil press. Installation, associated wiring, performance testing and commissioning remain included in the Supplier’s scope.

	Item No. 5
	Exception to the Factory-Manufactured Equipment Requirement
In Section VII – Schedule of Requirements, 3. Technical Specifications, please replace the equipment manufacturing requirement introduced under Item No. 4 of Amendment No. 1 with:
“All equipment shall be new and unused and shall meet the applicable technical requirements and international standards. Except for the oil press, equipment shall be certified and factory-manufactured, and locally fabricated machines shall not be acceptable. The oil press shall be locally fabricated in accordance with Item No. 4 of this Amendment.”
Clarification Q4 is superseded to the extent that it prohibits locally fabricated oil presses. The exception applies only to the oil press.

	Item No. 6
	Replacement of Technical Specifications and Bill of Quantities
In Section VII – Schedule of Requirements, please replace the Summary of Technical Specifications and the equipment and Combined Shared Solar System BOQs with Annex 1 – Revised Technical Specifications and Bills of Quantities, attached to and forming an integral part of this Amendment.
The revised solar arrangement comprises:
· A shared machinery system with thirty-six (36) 645 W panels, one 22 kW three-phase solar inverter, individual VFDs for the four machines, and the specified distribution, protection and control arrangements.
· A separately wired lighting/fan system with four (4) 645 W panels and one 3 kVA inverter.
The machinery shall operate in rotation, with only one machine running at a time. The shared machinery solar system shall be suitable for direct daytime operation without battery storage.
Solar BOQ quantities are stated per hub. Bidders shall include complete installations for all six (6) hubs.
The previous solar BOQ, including its hybrid inverter, battery and motor-drive arrangement, is superseded in its entirety.

	Item No. 7
	Solar Integration and Compliance with the Revised BOQ
In Section VII – Schedule of Requirements, 2. List of Related Services and Completion Schedule, Item No. 3, please replace:
“Installation, connection, and integration of the agro-processing equipment with the Employer-provided Solar PV system”
with
“Installation, connection, and integration of the agro-processing equipment with the Supplier-provided shared Solar PV system, including the separately wired solar system for lighting and fans, in accordance with the revised BOQ.”
For Clarification Q5, the BOQ and solar capacities specified in this Amendment shall replace the previous requirements. Bidders shall comply with the revised BOQ; further reductions in the specified solar capacities or alternative redesigns are not permitted.
The Supplier shall provide complete and compatible installations, including all equipment, connections, controls, protection, accessories, testing and commissioning necessary for the systems to operate as specified.

	Item No. 8
	Corresponding Bid and Price Schedule References
Bidders shall use the amended equipment names, motor ratings, quantities and solar requirements in their technical submissions and price schedules. Offers shall cover all six (6) hubs, including the required equipment, installation, integration, testing, commissioning, operator training, warranty support and handover.
The six (6)-week delivery and completion period established under Amendment No. 1 remains unchanged.

	Item No. 9 
	Delete Item No. 2 of Amendment No. 2 in its entirety.

	
	Attachment: Annex 1 – Revised Technical Specifications and Bills of Quantities.
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