	Name of Tender:
SD-CRS-538606-CW-RFQ / Provision of SC infrastructure rehabilitation/improvement works, including waste management - in Central Darfur.
Tender Number SD-CRS-538606-CW-RFQ
 Publish date: 27th of September 2026 
Deadline Submission date:
    08th of October 20262026 – 04 :00 PM
Please submit your bid to CRS Zalingei or
 through E/mail 
through email:  tenders.sudan@crs.org  
	اسم العطاء:
 أعمال إعادة تأهيل/تحسين البنية التحتية للخدمات الأساسية، بما في ذلك إدارة النفايات - في وسط دارفور.
رقم العطاء
 SD-CRS-538606-CW-RFQ

 تاريخ فتح التقدي  27 سبتمبر2026 
تاريخ انتهاء التقديم  8  كتوبر 2026 04:00   العصر 
 
الرجاء ارسال عرضكم الي مكتب الاغاثة الكاثلوكية زالنجي من خلال البريد الالكتروني 
tenders.sudan@crs.org 



 
 
	Dear Sir / Madam, 
CRS Sudan is looking for companies to provide the items/services shown in Attachment 1 at a competitive price and with high quality. 
 
General Requirements 
1.  Must Be Registered to conduct the business and in compliance with federal governments tax regulations in Sudan  
2.     Experience International Organizations, Non-Governmental Organizations, or large private companies will be an advantage.  
4.   CRS retains the right to reject, cancel, negotiate, amend, split and accept any offer, without consideration of the lowest offer. 
5.     This is an invitation to vendors, and it is not a promise or obligation that CRS will contract with suppliers through the submitted offers.
6.   Relevant bid committee may request for physical samples of some items during evaluation process of bids. 
7. The work plan must be provided by the contractor with the tender package.
9.The banking information should be specific and clear.


	 سيدي / سيدتي العزيز(ة)
هيئة الإغاثة الكاثوليكية  برامج السودان تبحث عن شركات من المهتمين بتوفير المواد/ الخدمات  المشار إليها أدناه في الملحق رقم 1 بأسعار منافسة وبجودة عالية.
متطلبات عامة:
1 . يجب أن يكون مسجلا لإجراء الأعمال التجارية مع ما يتوافق  ولوائح الضرائب الحكومية في السودان .
3 . الخبرة في تزويد المنظمات الدولية، المنظمات الغير حكومية، أو  الشركات الكبيرة الخاصة ستكون ميزة.
4 . تحتفظ هيئة الاغاثة الكاثوليكية بالحق في رفض، إلغاء، التفاوض، تعديل، تجزئة وقبول أي عرض، دون النظر الى أدنى عرض. .
5. هذه دعوة للموردين وليس وعد أو التزام من هيئة الإغاثة الكاثوليكية للتعاقد مع الموردين من خلال العروض المقدمة
6. قد تقوم لجنة الإحالة المعنية بطلب نماذج عينية لبعض المواد اثناء عملية تقييم العروض.
7.  يجب على المقاول تحضير الجدول الزمني لتنفيذ الاعمال على ان يتم تسليم المستند مع اوراق العطاء
9. يجب ان تكون معلومات وتفاصيل رقم الحساب واضحة.



 
	Payment Terms
1. Quotation should remain valid for a period of at least ninety (60) days from the submission closing date. 
2. Payment shall be made via bank cheque or wire transfer within 15 working days from the date of receiving the correct invoice.
3. Payment shall be made upon verification and acceptance of services according to contract    Purchase order. 

	     شروط الدفع :- 
يجب أن تظل العرض ساريًا لمدة تصل إلى تسعين (60) يومًا من تاريخ إغلاق التقديم.1
2. يتم إجراء الدفع عبر شيك بنكي أو تحويل بنكي خلال خمسة عشر (15) يوم عمل من تاريخ استلام الفاتورة الصحيحة.
3. يتم إجراء الدفع بعد التحقق وقبول الخدمات وفقًا لشروط العقد أو أمر الشراء



	Acceptance of Payment Terms
Do you accept the above payment terms?
· Yes
· No
 
	الموافقة على شروط الدفع:
هل توافق على شروط الدفع اعلاه:
· اوافق 
· لا اوافق 

	Requested Information
The submission must include:
· Full legal address and contact details of the company.
· Name of company’s official owner and copy of his/her ID & passport (if available)
· Copy of company registration certificate 
· Copy of Tax Registration Certificate.
· Reference from previous similar business experience with reference contact information. 
· Bank account information if available.
· The vendor must read, sign & stamp the Attachment (2) related to CRS SUPPLIER CODE OF CONDUCT
	يجب تقديم ما يلي:    
 يجب ان يتضمن التقديم ما يلي :                  
· العنوان الكامل الصحيح وعنوان الاتصال للشركة
· اسم صاحب الشركة الرسمي مع  نسخة من البطاقة القومية او جواز السفر.
· صورة عن شهادة تسجيل الشركة
· صورة عن شهادة التسجيل الضريبي 
· المرجع من الخبرة في الاعمال السابقة المماثلة و معلومات الاتصال للمرجع
· تفاصيل معلومات الحساب المصرفي اذا امكن.
· يجب على المقاول قراءة و توقيع و ختم الملحق(2) و الخاص بالقواعد السلوكية التي تنتهجها هيئة الإغاثة الكاثوليكية.


 
 
	Bid Requirements:- 
Offers that do not meet the following will be automatically rejected regardless of price:
1. Offers must be received before the stated deadline. 
2. Offers must include all the information requested above. 
3.  Unit prices must be provided for all line items. Offers that only include totals will be rejected..
4. Bids that include mistakes in calculations within the Bill of Quantities will be excluded from competition. 
5. Bids must be submitted through CRS Zalingei office to receive bids. 
6. Offers must be clean & clear. The vendor should sign and stamp next to handwritten corrections if available or corrections made with whiteout.  
7. Offers must be complete from all sides, signed, dated, and stamped on all pages. 
8. The technical adviser of CRS will carry out quality control of the items and reserve the right to reject and items did not match the above-mentioned specification.
9. The supplier Must be registered with MOH and present the documentation during tendering
10. The duration of delivery all requested items must be clearly specify 
	     
      معلومات ملء العطاء :- 
      سوف يتم رفض أي عطاء لا يلتزم بالشروط أدناه بغض النظر عن السعر:
1. سيتم رفض أي طلب يقدم بعد التاريخ والوقت المحدد لقبول العطاءات.
2. يجب أن تتضمن العروض جميع المعلومات المطلوبة أعلاه.
3. جميع الاسعار يجب ان تكتب لكل بند أو فقرة على حدة، ويتم رفض العطاءات التي تحتوي على الإجمالي فقط. 
4. سيتم استبعاد العطاء الذي يتضمن خطأ في حسابات جداول الكميات
5.  يجب تقديم العروض في مكتب المنظمة في   زالنجي  
6. العروض يجب أن تكون نظيفة وواضحة، يجب التوقيع والختم ان وجد في مكان أي تصحيح يدوي أو باستخدام قلم التصحيح الابيض.
7. يجب أن تكون العروض كاملة من جميع الجوانب، موقعة بتاريخ واضح ومختومة على جميع الصفحات.
8. سيقوم الجهة الفنية من قبل المنظمة لمطابقة المواصفات ويتم رفض أي دواء غير متطابق للمواصفات أعلاه.
9. يجب ان يكون العميل مسجل بوزارة الصحة واحضار المستندات 
10. يجب تحديد بشكل واضح  فترة تسليم كل الكميات المطلوبة 



 
	Delivery Instructions:
Complete and stamped and signed offer can be submitted directly to CRS Zalingei office. 
 
1. The company biography should not exceed 10 pages.
  
Complete and stamped and signed offer must be delivered in sealed envelope with tender number on it (SD-CRS-538606-CW-RFQ)  
Delivery to CRS Sudan office located in Zalingei 
	تعليمات التسليم: 
يجب تقديم العطاء الكامل والمختوم و الموقع  في مكتب زالنجي 
 
يجب ان لا تتجاوز السيرة الذاتية للشركة اكثر من 10 صفحات.
 
1. يجب تقديم العطاء الكامل والمختوم و الموقع  مع كافة الوثائق المطلوبة في  ظرف مغلق يكتب عليه رقم العطا (SD-CRS-538606-CW-RFQ) ويسلم الى مقر 
المنظمة في  زالنجي  
 
 




Experience Reference List
قائمة مراجع الاعمال السابقة
 
	 
	Name of Organization
أسم
المنظمة
	Name of Person
أسم الشخص
	Name of Project أسم المشروع
	Project Start Date تاريخ المباشرة بالمشروع
	Project duration مدة تنفيذ المشروع
	Phone Number رقم الموبايل
	Email Address البريد الالكتروني

	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 




	Company name:
أسم الشركة :
	 
 

	Legal address:
العنوان الثابت:
	 
 

	Telephone Number:
رقم الهاتف:
	 
 

	Email:
عنوان البريد الإلكتروني:
	 
 

	Representative Name
اسم الممثل:
	 
 

	Business Certificate Registration Number:
رقم تسجيل شهادة العمل:
	 

	Tax registration Number:
رقم التسجيل الضريبي:
	 

	Contract duration:
مدة العقد :
	 

	   Bank details: -

· Bank Name: ……………………………………

· Bank account name: …………………………

· Bank number ………………………………

· Branch: ………………………………………



  
	تفاصيل الحساب:- 

   إسم الينك : ----------------------------------------
 
اسم الحساب :----------------------------------------


رقم الحساب :  -------------------------------------  -  


الفرع -----------------------------------------------


	Do you have partnerships with any other companies (such as shared management / staff / office / bank account)?  Do you cooperate with any other companies in preparing offers or providing goods or services?
هل لديك شراكات مع أي من الشركات الأخرى ( مثل إدارة / الموظفين / المكتب حساب مشترك / البنك) ؟ هل تتعاون مع أي من الشركات الأخرى في إعداد العروض أو توفير السلع أو الخدمات؟
	 

	If the answer to the previous question is yes, please provide details here including the names of partner companies.
إذا كان الجواب عن السؤال السابق نعم ، يرجى تقديم التفاصيل هنا بما في ذلك أسماء الشركات الشريكة 
	 

	Other comments:
ملاحظات اخرى: 
	 

	Experience / references for the related work of experience (Please attached any related contract, purchase order, certificate, etc.) that does not exceed 10 pages. References MUST include contact information.  
يجب ان يحتوي على عناوين الاتصال من مراجع الخبرة 
المرجع من الخبرة ( الرجاء ارفاق دليل من الاعمال السابقة ذات الصلة من عقود , اوراق شراء , ورقة اتمام عمل , اخرى )  لا تتجاوز عشرة اوراق.
	 
 
 
 
 





	Signature
التوقيع
	 

	Date
التاريخ
	 





















                                                                    ATTACHED (1)  
                                                                      Specifications 
Central Dar fur      -    Mukjar  health facility
	A. Priority rehabilitation is required for ( OTP+TSFP, SC, EPI, Maternity ward, Dressing, Store, Dispensary and consultation office.

	No
	Items descriptions
	UOM
	QTY
	Unit price in SDG
	Total Price in SDG

	1
	Provide materials and close the zinc sheet's holes by using Refcoat and Damouria cloth for all medical services areas
	job
	job
	
	

	2
	Provide materials and repair all floors, using cement mortar mix 1:4 for all medical services areas
	job
	 job 
	
	

	3
	Provide materials and repair the main gates for the HF
	pcs
	         2.0 
	
	

	4
	Provide materials and repair the doors for all medical services areas
	pcs
	       20.0 
	
	

	5
	Provide materials and repair the windows for all medical services area
	pcs
	       39.0 
	
	

	6
	Provide and fix the missing windows for SC including paint
	pcs
	         3.0 
	
	

	7
	Provide and make stair for the main door of SC
	job
	 job 
	
	

	8
	Provide materials and repair the cracks for all medical services area, using concrete mix 1:2:4, steel bar 12mm with good curing three times per day.
	job
	 job 
	
	

	9
	Repair and review of electricity lines for all medical services areas including providing and fix the missing materials (lights, socket, and switch or all items using for electricity.
	job
	 job 
	
	

	10
	Provide material and rehabilitate of OTP's waiting area by removing the roof and change 30% of zinc sheet and metallic pipe including the provide and fix 1 door and 2 windows (3*1.25 m) + painting the wall internal and external.
	job
	 job 
	
	

	11
	Provide and make painting internal and external for SC using Bomastic Engineer Chemi Plast & Silk three face including the CRS's LOGOs .
	m2
	     250.0 
	
	

	12
	Provide and rehabilitate the waiting area for SC BY closing the sides using hard mesh, pipes 3*6 cm including the repair of plastering and provide and fix door
	job
	 job 
	
	

	13
	Provide materials and install solar system for SC including 2 panels 620 w, 2 battery 200V and inverter 3 kilo and all accessories.
	job
	 job 
	
	

	14
	Provide and fix heat isolation for SC 
	m2
	       70.0 
	
	

	Water and Sanitation (Latrine , Waste zone and Water Supply) - Priority rehabilitation is required for

	1
	 Repair the old incinerator and provide the damaged ventilation pipe, cover, and gate including of remove all soil over the pits.
	job
	 job 
	
	

	2
	Provide and fix ventilation pipe for the placenta pit and repair the wall of waste zone including the cracks and door
	job
	 job 
	
	

	3
	Excavate Sharp pit (1.5 m × 1.5 m ×3 m), and Ash pit (1.5 m × 1.5 m ×3 m) with provide the materials and build those pits using small bricks (first class), cement sand mortar with cover the pits  from the reinforced concrete including the mainahole with cover and ventilation pipe. including the repair of fence.
	job
	 job 
	
	

	4
	Provide and install water tank 1000 L for the maternity ward including the build of platform by dimension (1.5 L*1.2 W *1.5 H) , using 1.5 small bricks, cement sand mortar, concrete 10 cm thickness over the platform, filling the gaps with sand and plastering.
	job
	 job 
	
	

	5
	Tap stands with 1" GI outlet, support pedestal, apron slab + Plumbing Materials: GI pipe 1" (medium duty) + 1" Gate valves (brass) + Elbows, reducers, sockets, T-joints (assorted GI fittings) + PTFE tape & sealing compounds including the review of all lines from water source to the maternity ward with repair the soap pit.
	job
	 job 
	
	

	6
	Provide and fix handwashing facility for the medical service area and latrine including the good drainage of water using tank 50 L with metallic based.
	pcs
	         8.0 
	
	

	Constructing new wainting area shelter + Kitchen for SC

	1
	Excavate strip foundation with width 60 cm and depth 60 cm and back fill with stone up to level 40 cm 
	ml
	25.5
	
	

	2
	Excavate strip foundation with width 50 cm and depth 50 cm and back fill with stone up to level 30 cm for attached waiting Area shelter
	ml
	29
	
	

	3
	provide and construct   brick wall using thickness two brick (first class burn brick size 11cm x6cm x22 cm) with Hight 20 cm above Zero level, use cement/sand mix 1:8
	ml
	25.5
	
	

	4
	provide and construct   brick wall using thickness one and half brick (first class burn brick size 11cm x6cm x22 cm) with Hight 30 cm above Zero level, use cement/sand mix 1:8 for attached waiting Area shelter 
	ml
	29
	
	

	5
	provide and construct and cast reinforced concrete (1:2:4) mix for grade beam with section 30 cmx 30 cm use steel bar 12 mm 5T12@150mmc/c As shown in drawing
	ml
	25.5
	
	

	6
	provide and construct and cast reinforced concrete (1:2:4) mix for lentil beam with section 35 cmx 15 cm use steel bar 12 mm 5T12@150mmc/c As shown in drawing
	ml
	25.5
	
	

	7
	provide and construct and build brick walls including Barbate   by using thickness one and half brick (first class burn brick size 11cm x6cm x22 cm) ,use mud mortar
	m2
	102
	
	

	8
	Provide and construct brick wall 25 cm thickness with supports each 2 m using cement /sand mortar Mix   ( 1: 6 ) for waiting Area shelter
	m2
	35
	
	

	9
	provide and back filling using selected soil with well compacted in 3 layers for both room and attached waiting Area shelter
	m2
	26
	
	

	10
	Provide and casting plain concrete with 10 cm thickness with curing using water for 7 days for both room and attached waiting Area shelter
	m2
	72
	
	

	11
	provide and fix roof using UK zinc sheet(0.35mm) and Iron pipe 4 cm X 8 cm, 1mm thickness              as shown in drawing for both room and attached waiting Area shelter
	m2
	80
	
	

	12
	provide and install zinc sheet on upper side of shelter Hanging 100 cm using (American sheets)
	Meter Length(ML)
	29
	
	

	13
	provide and fix cylindrical iron pipe 3 inches in diameter , 3.5 m length and 1mm thickness for shelter witt painting
	Pcs
	14
	
	

	14
	Provide and plaster wall using cement/sand mortar mix 1:8 or both room and attached waiting Area shelter
	m2
	274
	
	

	15
	Provide and painting wall 2coat for External and internal wall using Bomastic paint or both room and attached waiting Area shelter
	m2
	274
	
	

	16
	Provide and fix  mesh (sixbenda) wit section 2 m length and 1 m height on shelter side 
	Pcs
	15
	
	

	17
	Provide and fix Doors with section 2 m X 1 m for shelter
	Pcs
	1
	
	

	18
	 provide and fix steel door size 1 mx2.2 m(accomy) with 20 cm opening in upper side covered by fiber using screw 
	Pcs
	2
	
	

	19
	 provide and fix steel window with fine mesh and sixbanda  size 1 mx1.2 m(accomy) with 20 cm opening in upper side covered by fiber using screw 
	Pcs
	3
	
	

	20
	 provide and fix sky light with fine mesh and sixbanda size 40 cm x 40 cm 
	pcs
	2
	
	

	Construction of short staying room (7 X 5 m) for SC

	1
	Excavate of strip foundation (0.50m width X0.80m depth) for short staying room and cart away the excavated soil from the site
	ML
	26
	
	

	2
	Supply and construct of stone strip footing (0.50m x 0.80m) in C/S mortar 1:6 mix for short staying room foundation as per drawings and specifications
	ML
	       24.0 
	
	

	3
	Supply and build walls with 2 Red bricks from mud mortar over the stone foundation for the height of 30 cm
	ML
	       24.0 
	
	

	4
	Supply, Installing and casting G.B 35×20Ccm from reinforcement concrete mixing 1:2:4 using 4 steel bars ,12 mm and 6mm as  specifications and drawings
	ML
	       24.0 
	
	

	5
	Backfilling under ground floor plain concrete with selected material approved by the engineer, Filling material shall be clean desert or drift soil filling should be in layers not exceeding 0.20 m watered and well compacted
	M3
	       10.5 
	
	

	6
	Supply and build Walls with 1.5 Red bricks and mud mortar up to 4.0 m above ground level to the roof including  the prabet
	M2
	       96.0 
	
	

	7
	Supply, Installing and casting T.B 35×15Ccm from reinforcement concrete mixing 1:2:4 using 4 steel bars ,12 mm and 6mm as  specifications and drawings
	ML
	       24.0 
	
	

	8
	Supply and fix of Corrugated zinc sheets and truss roof 0.4mm (caliber 35) with proper overlapping and fixed to purlins of 4x8 cm steel box section with screws. Price shall include fixing ridge cap in truss top. Purlins number and spacing as per drawings, the work should also include installation of isolation sheets under the zinc sheets
	M2
	       35.0 
	
	

	9
	Supply and cast 7cm thick plain concrete 1:3:6 mix with approved ordinary port land cement and approved coarse and sand for all flooring
	M2
	       35.0 
	
	

	10
	Supply and fix plastering for internal walls & external walls using C/S mortar mix 1:8 & 1:6 as per specifications
	M2
	     192.0 
	
	

	11
	Provide and make painting for internal walls & external walls using Bomastic Engineer Chemi Plast & Silk three faces including the CRS's LOGOs .
	M2
	     192.0 
	
	

	12
	Provide and fix steel door 2.2x1.2 using steel rectangular 4 x 8 cm and 3 x 6 cm as per drawings and including the handles and blocks and including the painting works.
	pcs
	         1.0 
	
	

	13
	Provide and fix steel Windows 1.2 m x 0.9 m using rectangular steel 3 x6 inches and 3 x 6 inches as per drawings and including the handles and blocks and including the painting works
	pcs
	         7.0 
	
	

	14
	Provide and connect electricity for the short staying room including fans, lights, socket, and switch or all items using for electricity.
	job
	 job 
	
	

	
	SUM
	
	
	
	

	
	







	
Bidder’s (Company) Name: ________________

Authorized Person Full Name: _____________
Title (Position):	_________________________

Signature and Company Official Stamp:	_____

Date: ____________________

	
اسم مقدم العرض (الشركة)___________________

الاسم الكامل للشخص المفوض: _________________ 

اللقب (المنصب): ___________________________

التوقيع وختم الشركة الرسمي: _______________

التاريخ:___________________________







